
New TopShim run:

version = topshim 4.4.0
date = 2025-11-18
time = 00:28:14.388
command = topshim tunebxyz tuneaz ordmax=6

FINE SHIMMING

Parameters:

probe = Z113652_0123
solvent = DMSO
shim nucleus = 2H
nucleus optimised for = 1H
o1p (from lock) = 2.49 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 1.3 Hz, Target= 0.3 Hz, After= 0.3 Hz
Iteration 2: FWHM Before= 0.3 Hz, Target= 0.4 Hz, After= 0.4 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.489


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	-549
Z2	-24
Z3	+47
Z4	+584
Z5	-138
Z6	-1811

duration = 1 min 20 sec
completed successfully
finished Tue Nov 18 00:29:33 2025


========================================================================
