
New TopShim run:

version = topshim 4.4.0
date = 2025-12-01
time = 16:48:35.437
command = topshim 1d ls coil=1H ls tuneaoff lockoff 1h o1p=2.76 selwid=0.5 ordmax=6

FINE SHIMMING

Parameters:

probe = Z113652_0123
solvent = CDCl3
shim nucleus = 1H
nucleus optimised for = 1H
o1p (set) = 2.76 ppm
selective excitation width = 0.5 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 0.9 Hz, Target= 0.2 Hz, After= 0.4 Hz
Iteration 2: FWHM Before= 0.4 Hz, Target= 0.3 Hz, After= 0.4 Hz
Iteration 3: FWHM Before= 0.4 Hz, Target= 0.2 Hz, After= 0.2 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.376

shim changes: 
Z	-91
Z2	-15
Z3	-21
Z4	+101
Z5	-110
Z6	-166

duration = 18 sec
completed successfully
finished Mon Dec  1 16:48:52 2025


========================================================================
