
New TopShim run:

version = topshim 4.4.0
date = 2025-10-21
time = 14:25:25.836
command = topshim tunebxyz tuneaz ordmax=6

FINE SHIMMING

Parameters:

probe = Z113652_0123
solvent = CDCl3
shim nucleus = 2H
nucleus optimised for = 1H
o1p (from lock) = 7.24 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before=38.7 Hz, Target= 0.7 Hz, After= 0.5 Hz
Iteration 2: FWHM Before= 0.5 Hz, Target= 0.7 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.675


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	-471
Z2	+41
Z3	+15
Z4	+40
Z5	-66

duration = 1 min 14 sec
completed successfully
finished Tue Oct 21 14:26:39 2025


========================================================================
