
New TopShim run:

version = topshim 4.4.0
date = 2025-10-24
time = 17:34:06.145
command = topshim tunebxyz tuneaz ordmax=6

FINE SHIMMING

Parameters:

probe = Z113652_0123
solvent = CDCl3
shim nucleus = 2H
nucleus optimised for = 1H
o1p (from lock) = 7.24 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before=55.8 Hz, Target= 0.3 Hz, After= 0.9 Hz
Iteration 2: FWHM Before= 0.9 Hz, Target= 0.4 Hz, After= 0.4 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.602


Performing tune after shimming
tune lock level increase = 1.1

shim changes: 
Z	-670
Z2	+28
Z3	-3
Z4	-705
Z5	-331
Z6	+674

duration = 1 min 30 sec
completed successfully
finished Fri Oct 24 17:35:35 2025


========================================================================
