
New TopShim run:

version = topshim 4.4.0
date = 2025-11-05
time = 06:32:55.315
command = topshim tunebxyz tuneaz ordmax=6

FINE SHIMMING

Parameters:

probe = Z113652_0123
solvent = CDCl3
shim nucleus = 2H
nucleus optimised for = 1H
o1p (from lock) = 7.24 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before=19.3 Hz, Target= 0.6 Hz, After= 0.3 Hz
Iteration 2: FWHM Before= 0.3 Hz, Target= 0.3 Hz, After= 0.5 Hz
Iteration 3: FWHM Before= 0.5 Hz, Target= 0.4 Hz, After= 0.4 Hz
Iteration 4: FWHM Before= 0.4 Hz, Target= 0.5 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.529


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	-366
Z2	+83
Z3	-8
Z4	-315
Z5	-119
Z6	+902

duration = 1 min 26 sec
completed successfully
finished Wed Nov  5 06:34:20 2025


========================================================================
