
New TopShim run:

version = topshim 4.4.0
date = 2025-11-16
time = 04:18:49.455
command = topshim tunebxyz tuneaz ordmax=6

FINE SHIMMING

Parameters:

probe = Z113652_0123
solvent = CDCl3
shim nucleus = 2H
nucleus optimised for = 1H
o1p (from lock) = 7.24 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before=30.6 Hz, Target= 0.5 Hz, After= 0.6 Hz
Iteration 2: FWHM Before= 0.6 Hz, Target= 0.3 Hz, After= 0.4 Hz
Iteration 3: FWHM Before= 0.4 Hz, Target= 0.4 Hz, After= 0.7 Hz
Iteration 4: FWHM Before= 0.7 Hz, Target= 0.6 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.711


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	-504
Z2	+74
Z3	-3
Z4	-263
Z5	-114
Z6	+726

duration = 1 min 28 sec
completed successfully
finished Sun Nov 16 04:20:16 2025


========================================================================
