
New TopShim run:

version = topshim 4.4.0
date = 2025-10-24
time = 10:42:43.608
command = topshim tunebxyz tuneaz ordmax=6

FINE SHIMMING

Parameters:

probe = Z113652_0123
solvent = CDCl3
shim nucleus = 2H
nucleus optimised for = 1H
o1p (from lock) = 7.24 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 1.9 Hz, Target= 0.8 Hz, After= 0.5 Hz
Iteration 2: FWHM Before= 0.5 Hz, Target= 0.4 Hz, After= 0.3 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.466


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	-467
Z2	+91
Z3	+30
Z4	-285
Z5	-100
Z6	+823

duration = 1 min 24 sec
completed successfully
finished Fri Oct 24 10:44:07 2025


========================================================================
