
New TopShim run:

version = topshim 4.4.0
date = 2025-11-05
time = 21:00:58.221
command = topshim tunebxyz tuneaz ordmax=6

FINE SHIMMING

Parameters:

probe = Z113652_0123
solvent = CDCl3
shim nucleus = 2H
nucleus optimised for = 1H
o1p (from lock) = 7.24 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before=11.1 Hz, Target= 0.5 Hz, After= 0.3 Hz
Iteration 2: FWHM Before= 0.3 Hz, Target= 0.3 Hz, After= 0.4 Hz
Iteration 3: FWHM Before= 0.4 Hz, Target= 0.3 Hz, After= 0.3 Hz
Iteration 4: FWHM Before= 0.3 Hz, Target= 0.3 Hz, After= 0.6 Hz
Iteration 5: FWHM Before= 0.6 Hz, Target= 0.4 Hz, After= 0.5 Hz
Iteration 6: FWHM Before= 0.5 Hz, Target= 0.3 Hz, After= 0.4 Hz
Iteration 7: FWHM Before= 0.4 Hz, Target= 0.3 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.483


Performing tune after shimming
tune lock level increase = 1.0

shim changes: 
Z	-376
Z2	+80
Z3	-8
Z4	-419
Z5	-87
Z6	+1131

duration = 1 min 50 sec
completed successfully
finished Wed Nov  5 21:02:47 2025


========================================================================
