
New TopShim run:

version = topshim 4.4.0
date = 2026-03-27
time = 11:25:07.793
command = topshim 1d ls coil=1H ls tuneaoff ordmax=6

FINE SHIMMING

Parameters:

probe = Z113652_0123
solvent = CDCl3
shim nucleus = 2H
nucleus optimised for = 1H
o1p (from lock) = 7.24 ppm

Results:


1D Shimming:
Iteration 1: FWHM Before= 4.9 Hz, Target= 0.4 Hz, After= 0.5 Hz
Iteration 2: FWHM Before= 0.5 Hz, Target= 0.4 Hz, After= 0.3 Hz
Shim succeeded

Lineshape quality factor (1D spectrum, spinning) = 0.522

shim changes: 
Z	-35
Z2	+17
Z3	-39
Z4	-249
Z5	+5
Z6	+696

duration = 48 sec
completed successfully
finished Fri Mar 27 11:25:55 2026


========================================================================
