CONFIGURATION INFORMATION
=========================

Path         : C:/Bruker/TopSpin3.2pl7/conf/instr/FOURIER300/uxnmr.info
Date         : Mon May 19 09:33:10 2025
Release      : TOPSPIN Version 3.2-pl7
Installed in : C:/Bruker/TopSpin3.2pl7
Host         : FOURIER-300
OS           : Windows 7 (Vs 6.1) Service Pack 1
CPU          : Intel(R) Xeon(R) CPU E5-1620 v3 @ 3.50GHz (8 cores at 3491 MHz with Hyperthreading)
User         : nmrsu
Description  : FOURIER300
Location     : UBA - Chemistry
System       : Fourier NMR spectrometer
1H-frequency : 300.18 MHz
Order Number : 10203718
Configured in: C:/Bruker/TopSpin3.2pl7/conf/instr/FOURIER300

AcqControlServer: DRMS DRU 
- TCP/IP address = 127.0.0.1
- Firmware Version = 29259

Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
Minispec Amplifier HMG01/215 ECL 200:
- TCP/IP address = 149.236.99.254
- Amplifier      = DrmsTrmX: HMG01/215 ECL 200
Minispec Amplifier HMG02/215 ECL 200:
- TCP/IP address = 149.236.99.254
- Amplifier      = DrmsTrmH: HMG02/215 ECL 200

BSMS: Fourier Magnet Controller connected to ethernet
- TCP/IP address = 149.236.99.253

Sample Changers at the spectrometer subnet:
-------------------------------------------
 - BACS2_H15200_719: at TCP/IP address 149.236.99.200


VTUs at the spectrometer subnet:
--------------------------------
Fourier Variable Temperature Unit :
- TCP/IP address   = 149.236.99.252

Preamplifiers :
Minispec Preamplifier configured via Minispec BIS
    Module  1 : preamplifier module 1
     Module Name    : Drms13C
     Part/Serialno  : HMG03/01389
     Observe Nuclei : 13C
     Lock Nuclei    : 2H, 19F
    Module  2 : preamplifier module 2
     Module Name    : Drms1H
     Part/Serialno  : HMG04/01389
     Observe Nuclei : 1H
     Lock Nuclei    : 2H, 19F
    Module  3 : preamplifier module 3
     Module Name    : Drms2H
     Part/Serialno  : HMG05/01389
     Observe Nuclei : 2H
     Lock Nuclei    : 2H, 19F


